<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="140" y2="0" width="0" layer="20"/>
<wire x1="140" y1="0" x2="140" y2="100" width="0" layer="20"/>
<wire x1="140" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<text>RESET</text>
<text>RFID Transponder</text>
<text>RTS</text>
<text>D1</text>
<text>D0</text>
<text>UPDI</text>
<text>SDA</text>
<text>SCL</text>
<text>rev 1</text>
<text>JLCJLCJLCJLC</text>
<text>5V</text>
<text>GND</text>
<text>GPIO</text>
<text>3,3V</text>
<text>CLK</text>
<text>CS</text>
<text>MISO</text>
<text>MOSI</text>
<text>GND</text>
<text>5V</text>
<text>Designed by Ruben Schoonbaert</text>
<text>ESD sensitive!</text>
<text>Caution,</text>
<hole x="132" y="8" drill="3.3"/>
<text>GPIO</text>
<text>TTL Flash &amp; UPDI</text>
<text>Micro-SD</text>
<text>POWER</text>
<hole x="8" y="92" drill="3.3"/>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CAPC2012X145N">
<description>&lt;b&gt;GRM21_0.10 L=2.0mm W=1.25mm T=1.25mm&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CAPC2012X94N">
<description>&lt;b&gt;08055C104KAT2A&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CAPPM3216X180N">
<description>&lt;b&gt;CASE A&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="T491A">
<description>&lt;b&gt;T491A-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="FUSC2114X125N">
<description>&lt;b&gt;SMD0805B050TF&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOIC127P600X175-8N">
<description>&lt;b&gt;SO8N&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOP65P640X110-14N">
<description>&lt;b&gt;SOT402-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="1016435900011LF">
<description>&lt;b&gt;10164359-00011LF-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="849528">
<description>&lt;b&gt;84952-8-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="LEDC2012X80N">
<description>&lt;b&gt;SML-LXT0805GW-TR&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="RESC2012X50N">
<description>&lt;b&gt;CRCW0805&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="RESC2012X60N">
<description>&lt;b&gt;RC0805FR&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="RESC2012X65N">
<description>&lt;b&gt;RNCP0805_2021&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOD3716X145N">
<description>&lt;b&gt;SOD123-ren1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="MEM20750014001A">
<description>&lt;b&gt;MEM2075-00-140-01-A-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CMT-8540S-SMT-TR">
<description>&lt;b&gt;CMT-8540S-SMT-TR&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="PTS636SM50SMTRLFS">
<description>&lt;b&gt;PTS636 SM50 SMTR LFS-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="crystal-geyer_V1_0">
<description>&lt;BR&gt;&lt;big&gt;&lt;b&gt;GEYER ELECTRONIC --- Your producer for quartz crystals and oscillators&lt;/B&gt;&lt;/big&gt;&lt;br&gt;&lt;Hr&gt;

Version 1.0, 07.06.2016
&lt;hr&gt;
&lt;BR&gt;&lt;BR&gt; 

&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;GEYER ELECTRONIC e.K.&lt;/b&gt;&lt;br&gt;


Lochhamer Schlag 5&lt;br&gt;
D-82166 Gräfelfing/München&lt;br&gt;
&lt;br&gt;
Tel:   +49 89 546868-0&lt;br&gt;
Fax: +49 89 546868-90 für Batterien und Ladetechnik&lt;br&gt;
Fax: +49 89 546868-91 für Quarzprodukte&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.geyer-electronic.de"&gt;http://www.geyer-electronic.de&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:info@geyer-electronic.de"&gt;info@geyer-electronic.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor Geyer-Electronic does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Copyright: Geyer-Electronic</description>
<packages>
<package name="3.2X1.5">
<description>2 Pad</description>
</package>
</packages>
</library>
<library name="ATMEGA3208-AFR">
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="AMS1117-3.3">
<packages>
<package name="SOT229P700X180-4N">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP09R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mijn-library">
<packages>
<package name="RF_COIL">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0805" value="18pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C10" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="SamacSys_Parts" package="CAPC2012X94N" value="08055C104KAT2A">
<attribute name="DESCRIPTION" value="0805 X7R ceramic capacitor,100nF 50V AVX 0805 Standard 100nF Ceramic Multilayer Capacitor, 50 V dc, +125degC, X7R Dielectric,  /-10% SMD"/>
<attribute name="HEIGHT" value="0.94mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="08055C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-08055C104K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/08055C104KAT2A?qs=2ujN4bDBNE9mJvapP%252BjopA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C12" library="SamacSys_Parts" package="CAPPM3216X180N" value="TAJA106K010YNJ">
<attribute name="DESCRIPTION" value="Tantalum Capacitors - Solid SMD 10volts 10uF 10%"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TAJA106K010YNJ"/>
<attribute name="MOUSER_PART_NUMBER" value="581-TAJA106K010YNJ"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=581-TAJA106K010YNJ"/>
<attribute name="NAME"/>
</element>
<element name="C13" library="SamacSys_Parts" package="CAPC2012X94N" value="08055C104KAT2A">
<attribute name="DESCRIPTION" value="0805 X7R ceramic capacitor,100nF 50V AVX 0805 Standard 100nF Ceramic Multilayer Capacitor, 50 V dc, +125degC, X7R Dielectric,  /-10% SMD"/>
<attribute name="HEIGHT" value="0.94mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="08055C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-08055C104K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/08055C104KAT2A?qs=2ujN4bDBNE9mJvapP%252BjopA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C14" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="SamacSys_Parts" package="CAPC2012X94N" value="08055C104KAT2A">
<attribute name="DESCRIPTION" value="0805 X7R ceramic capacitor,100nF 50V AVX 0805 Standard 100nF Ceramic Multilayer Capacitor, 50 V dc, +125degC, X7R Dielectric,  /-10% SMD"/>
<attribute name="HEIGHT" value="0.94mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="08055C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-08055C104K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/08055C104KAT2A?qs=2ujN4bDBNE9mJvapP%252BjopA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0805" value="18pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C3" library="SamacSys_Parts" package="T491A" value="T491A226K004AT">
<attribute name="DESCRIPTION" value="T491, Tantalum, MnO2 Tantalum, Commercial Grade, 22 uF, 10%, 4 VDC, 125C, -55C, 85C, SMD, MnO2, Molded, 6 % , 3.5 Ohms, 900 nA, 58.6 mg, 3216, 1.6mm, Height Max = 1.8mm, 2000, 156  Weeks"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="MANUFACTURER_NAME" value="KEMET"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="T491A226K004AT"/>
<attribute name="MOUSER_PART_NUMBER" value="80-T491A226K004AT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=80-T491A226K004AT"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="SamacSys_Parts" package="CAPC2012X94N" value="08055C104KAT2A">
<attribute name="DESCRIPTION" value="0805 X7R ceramic capacitor,100nF 50V AVX 0805 Standard 100nF Ceramic Multilayer Capacitor, 50 V dc, +125degC, X7R Dielectric,  /-10% SMD"/>
<attribute name="HEIGHT" value="0.94mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="08055C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-08055C104K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/08055C104KAT2A?qs=2ujN4bDBNE9mJvapP%252BjopA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="SamacSys_Parts" package="CAPC2012X94N" value="08055C104KAT2A">
<attribute name="DESCRIPTION" value="0805 X7R ceramic capacitor,100nF 50V AVX 0805 Standard 100nF Ceramic Multilayer Capacitor, 50 V dc, +125degC, X7R Dielectric,  /-10% SMD"/>
<attribute name="HEIGHT" value="0.94mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="08055C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-08055C104K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/08055C104KAT2A?qs=2ujN4bDBNE9mJvapP%252BjopA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="SamacSys_Parts" package="CAPC2012X94N" value="08055C104KAT2A">
<attribute name="DESCRIPTION" value="0805 X7R ceramic capacitor,100nF 50V AVX 0805 Standard 100nF Ceramic Multilayer Capacitor, 50 V dc, +125degC, X7R Dielectric,  /-10% SMD"/>
<attribute name="HEIGHT" value="0.94mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="08055C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-08055C104K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/08055C104KAT2A?qs=2ujN4bDBNE9mJvapP%252BjopA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="F1" library="SamacSys_Parts" package="FUSC2114X125N" value="SMD0805B050TF">
<attribute name="DESCRIPTION" value="Resettable Fuses - PPTC PPTC 6V 0.5A"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SMD0805B050TF"/>
<attribute name="MOUSER_PART_NUMBER" value="603-SMD0805B050TF"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/SMD0805B050TF?qs=0lSvoLzn4L91PoLHRQNgaQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="SamacSys_Parts" package="SOIC127P600X175-8N" value="ST25DV16KC-IE6S3">
<attribute name="DESCRIPTION" value="Dynamic NFC/RFID tag IC with 16-Kbit EEPROM, and fast transfer mode capability"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ST25DV16KC-IE6S3"/>
<attribute name="MOUSER_PART_NUMBER" value="511-ST25DV16KC-IE6S3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/ST25DV16KC-IE6S3?qs=QNEnbhJQKvbFHl9iSDOFGA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="SamacSys_Parts" package="SOP65P640X110-14N" value="74LVC125APW,118">
<attribute name="DESCRIPTION" value="74LVC125A - Quad buffer/line driver with 5 V tolerant input/outputs; 3-state@en-us"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="Nexperia"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="74LVC125APW,118"/>
<attribute name="MOUSER_PART_NUMBER" value="771-74LVC125APW-T"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC125APW118?qs=me8TqzrmIYV8VAZOS5KVLw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SamacSys_Parts" package="1016435900011LF" value="10164359-00011LF">
<attribute name="DESCRIPTION" value="USB Type C Receptacle SMT Single Row 6Pin"/>
<attribute name="HEIGHT" value="3.41mm"/>
<attribute name="MANUFACTURER_NAME" value="Amphenol"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="10164359-00011LF"/>
<attribute name="MOUSER_PART_NUMBER" value="649-10164359-00011LF"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Amphenol-FCI/10164359-00011LF?qs=MyNHzdoqoQLpQ%2FmSqA1%252BtQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="SamacSys_Parts" package="849528" value="84952-8">
<attribute name="DESCRIPTION" value="8 way r/a bottom FFC SMT connector,1mm"/>
<attribute name="HEIGHT" value="2.74mm"/>
<attribute name="MANUFACTURER_NAME" value="TE Connectivity"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="84952-8"/>
<attribute name="MOUSER_PART_NUMBER" value="571-84952-8"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity/84952-8?qs=uUkeXfjQ8uTKEYAHE0dNDQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="SamacSys_Parts" package="LEDC2012X80N" value="SML-LXT0805GW-TR">
<attribute name="DESCRIPTION" value="LED,0805,Surface Mount,QuasarBrite Lumex SML-LXT0805GW-TR Green LED, 565 nm, 0805 Diffused, Rectangle Lens SMD Package"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Lumex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SML-LXT0805GW-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="696-SML-LXT0805GW"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Lumex/SML-LXT0805GW-TR?qs=9HInCHf8eFiVOx4SP694cA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="Q1" library="crystal-geyer_V1_0" package="3.2X1.5" value="32.768Khz">
<attribute name="NAME"/>
</element>
<element name="R1" library="SamacSys_Parts" package="RESC2012X50N" value="CRCW08053K30FKEA">
<attribute name="DESCRIPTION" value="CRCW0805 Resistor T/R 0.125W,1%,3K3 Vishay CRCW Series Thick Film Surface Mount Resistor 805 Case 3.3k +/-1% 0.125W +/-100ppm/C"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Vishay"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08053K30FKEA"/>
<attribute name="MOUSER_PART_NUMBER" value="71-CRCW0805-3.3K-E3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Vishay-Dale/CRCW08053K30FKEA?qs=kJXytlGtIWkHrvHHExLW2Q%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R10" library="SamacSys_Parts" package="RESC2012X60N" value="RC0805FR-0710KL">
<attribute name="DESCRIPTION" value="YAGEO - RC0805FR-0710KL - SMD Chip Resistor, 10 kohm, +/- 1%, 125 mW, 0805 [2012 Metric], Thick Film, General Purpose"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0805FR-0710KL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0805FR-0710KL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/RC0805FR-0710KL?qs=7bY8808IzHq6vrU3BeiiYw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R11" library="SamacSys_Parts" package="RESC2012X60N" value="RC0805FR-0710KL">
<attribute name="DESCRIPTION" value="YAGEO - RC0805FR-0710KL - SMD Chip Resistor, 10 kohm, +/- 1%, 125 mW, 0805 [2012 Metric], Thick Film, General Purpose"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0805FR-0710KL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0805FR-0710KL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/RC0805FR-0710KL?qs=7bY8808IzHq6vrU3BeiiYw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R12" library="SamacSys_Parts" package="RESC2012X60N" value="RC0805FR-0710KL">
<attribute name="DESCRIPTION" value="YAGEO - RC0805FR-0710KL - SMD Chip Resistor, 10 kohm, +/- 1%, 125 mW, 0805 [2012 Metric], Thick Film, General Purpose"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0805FR-0710KL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0805FR-0710KL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/RC0805FR-0710KL?qs=7bY8808IzHq6vrU3BeiiYw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SamacSys_Parts" package="RESC2012X50N" value="CRCW08053K30FKEA">
<attribute name="DESCRIPTION" value="CRCW0805 Resistor T/R 0.125W,1%,3K3 Vishay CRCW Series Thick Film Surface Mount Resistor 805 Case 3.3k +/-1% 0.125W +/-100ppm/C"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Vishay"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08053K30FKEA"/>
<attribute name="MOUSER_PART_NUMBER" value="71-CRCW0805-3.3K-E3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Vishay-Dale/CRCW08053K30FKEA?qs=kJXytlGtIWkHrvHHExLW2Q%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="SamacSys_Parts" package="RESC2012X50N" value="CRCW08053K30FKEA">
<attribute name="DESCRIPTION" value="CRCW0805 Resistor T/R 0.125W,1%,3K3 Vishay CRCW Series Thick Film Surface Mount Resistor 805 Case 3.3k +/-1% 0.125W +/-100ppm/C"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Vishay"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08053K30FKEA"/>
<attribute name="MOUSER_PART_NUMBER" value="71-CRCW0805-3.3K-E3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Vishay-Dale/CRCW08053K30FKEA?qs=kJXytlGtIWkHrvHHExLW2Q%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="SamacSys_Parts" package="RESC2012X50N" value="CRCW08053K30FKEA">
<attribute name="DESCRIPTION" value="CRCW0805 Resistor T/R 0.125W,1%,3K3 Vishay CRCW Series Thick Film Surface Mount Resistor 805 Case 3.3k +/-1% 0.125W +/-100ppm/C"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Vishay"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08053K30FKEA"/>
<attribute name="MOUSER_PART_NUMBER" value="71-CRCW0805-3.3K-E3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Vishay-Dale/CRCW08053K30FKEA?qs=kJXytlGtIWkHrvHHExLW2Q%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="SamacSys_Parts" package="RESC2012X60N" value="RC0805FR-0710KL">
<attribute name="DESCRIPTION" value="YAGEO - RC0805FR-0710KL - SMD Chip Resistor, 10 kohm, +/- 1%, 125 mW, 0805 [2012 Metric], Thick Film, General Purpose"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0805FR-0710KL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0805FR-0710KL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/RC0805FR-0710KL?qs=7bY8808IzHq6vrU3BeiiYw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="SamacSys_Parts" package="RESC2012X60N" value="RC0805FR-0710KL">
<attribute name="DESCRIPTION" value="YAGEO - RC0805FR-0710KL - SMD Chip Resistor, 10 kohm, +/- 1%, 125 mW, 0805 [2012 Metric], Thick Film, General Purpose"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0805FR-0710KL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0805FR-0710KL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/RC0805FR-0710KL?qs=7bY8808IzHq6vrU3BeiiYw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="SamacSys_Parts" package="RESC2012X65N" value="RNCP0805FTD1K00">
<attribute name="DESCRIPTION" value="RES, 1 Kohm, 0805, 1%, 100 ppm, 0.25W"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Stackpole Electronics, Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RNCP0805FTD1K00"/>
<attribute name="MOUSER_PART_NUMBER" value="708-RNCP0805FTD1K00"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/SEI-Stackpole/RNCP0805FTD1K00?qs=FESYatJ8odKy9z1hnQn%252Bhg%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="SamacSys_Parts" package="RESC2012X65N" value="RNCP0805FTD1K00">
<attribute name="DESCRIPTION" value="RES, 1 Kohm, 0805, 1%, 100 ppm, 0.25W"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Stackpole Electronics, Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RNCP0805FTD1K00"/>
<attribute name="MOUSER_PART_NUMBER" value="708-RNCP0805FTD1K00"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/SEI-Stackpole/RNCP0805FTD1K00?qs=FESYatJ8odKy9z1hnQn%252Bhg%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="SamacSys_Parts" package="RESC2012X60N" value="RC0805FR-0710KL">
<attribute name="DESCRIPTION" value="YAGEO - RC0805FR-0710KL - SMD Chip Resistor, 10 kohm, +/- 1%, 125 mW, 0805 [2012 Metric], Thick Film, General Purpose"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="YAGEO"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RC0805FR-0710KL"/>
<attribute name="MOUSER_PART_NUMBER" value="603-RC0805FR-0710KL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/YAGEO/RC0805FR-0710KL?qs=7bY8808IzHq6vrU3BeiiYw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="ATMEGA3208-AFR" package="QFP80P900X900X120-32N" value="ATMEGA3208-AFR">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/ATMEGA3208-AFR/Microchip/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value=" AVR megaAVR® 0, Functional Safety (FuSa) Microcontroller IC 8-Bit 20MHz 32KB (32K x 8) FLASH 32-TQFP (7x7) "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="ATMEGA3208-AFR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="TQFP-32 Microchip"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=2762707&amp;manufacturer=Microchip&amp;part_name=ATMEGA3208-AFR&amp;search_term=None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/ATMEGA3208-AFR/Microchip/view-part/?ref=snap"/>
</element>
<element name="D2" library="SamacSys_Parts" package="SOD3716X145N" value="MMSZ5231B-7-F">
<attribute name="DESCRIPTION" value="Zener Diode 5.1V 5% 500mW SOD123 Diodes Inc MMSZ5231B-7-F Zener Diode, 5.1V 5% 0.5 W SMT 2-Pin SOD-123"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MMSZ5231B-7-F"/>
<attribute name="MOUSER_PART_NUMBER" value="621-MMSZ5231B-F"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/MMSZ5231B-7-F?qs=2ygBApjwyeMh7Sf0YL1qSw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="SamacSys_Parts" package="CAPC2012X145N" value="GRM21BR61C106KE15K">
<attribute name="DESCRIPTION" value="Murata, 0805 (2012M) 10uF Multilayer Ceramic Capacitor MLCC 16V dc +/-10% , SMD GRM21BR61C106KE15K"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR61C106KE15K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM21BR61C106KE5K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM21BR61C106KE15K?qs=h0WOCFF19ULjTOS37upAEw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="SamacSys_Parts" package="849528" value="84952-8">
<attribute name="DESCRIPTION" value="8 way r/a bottom FFC SMT connector,1mm"/>
<attribute name="HEIGHT" value="2.74mm"/>
<attribute name="MANUFACTURER_NAME" value="TE Connectivity"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="84952-8"/>
<attribute name="MOUSER_PART_NUMBER" value="571-84952-8"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity/84952-8?qs=uUkeXfjQ8uTKEYAHE0dNDQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J4" library="SamacSys_Parts" package="MEM20750014001A" value="MEM2075-00-140-01-A">
<attribute name="DESCRIPTION" value="GCT (GLOBAL CONNECTOR TECHNOLOGY) - MEM2075-00-140-01-A - MICRO SD CARD CONN, PUSH-PUSH, 9POS, SMT"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="GCT (GLOBAL CONNECTOR TECHNOLOGY)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MEM2075-00-140-01-A"/>
<attribute name="MOUSER_PART_NUMBER" value="640-MEM20750014001A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/GCT/MEM2075-00-140-01-A?qs=KUoIvG%2F9IlZvfWpeERlq3Q%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="AMS1117-3.3" package="SOT229P700X180-4N" value="AMS1117-3.3">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/AMS1117-3.3/Advanced+Monolithic+Systems/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value=" Sot223/Pkg 1-Amp 3.3-Volt Low Drop Out Voltage Regulatator "/>
<attribute name="MF" value="Advanced Monolithic Systems"/>
<attribute name="MP" value="AMS1117-3.3"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-223 Seeed Technology"/>
<attribute name="PRICE" value="None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/AMS1117-3.3/Advanced+Monolithic+Systems/view-part/?ref=snap"/>
</element>
<element name="TP1" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP5" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LS1" library="SamacSys_Parts" package="CMT-8540S-SMT-TR" value="CMT-8540S-SMT-TR">
<attribute name="DESCRIPTION" value="MAGNETIC BUZZER TRANSDUCER, 4000 Hz"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="CUI Devices"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CMT-8540S-SMT-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="490-CMT-8540S-SMT-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CUI-Devices/CMT-8540S-SMT-TR?qs=qCxwlXJ4fnyb8bN8CSFJVw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R13" library="SamacSys_Parts" package="RESC2012X65N" value="RNCP0805FTD1K00">
<attribute name="DESCRIPTION" value="RES, 1 Kohm, 0805, 1%, 100 ppm, 0.25W"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Stackpole Electronics, Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RNCP0805FTD1K00"/>
<attribute name="MOUSER_PART_NUMBER" value="708-RNCP0805FTD1K00"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/SEI-Stackpole/RNCP0805FTD1K00?qs=FESYatJ8odKy9z1hnQn%252Bhg%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="D3" library="SamacSys_Parts" package="LEDC2012X80N" value="SML-LXT0805GW-TR">
<attribute name="DESCRIPTION" value="LED,0805,Surface Mount,QuasarBrite Lumex SML-LXT0805GW-TR Green LED, 565 nm, 0805 Diffused, Rectangle Lens SMD Package"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Lumex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SML-LXT0805GW-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="696-SML-LXT0805GW"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Lumex/SML-LXT0805GW-TR?qs=9HInCHf8eFiVOx4SP694cA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="TP7" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP9" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP10" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP11" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP12" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="testpad" package="TP09R" value="TPTP09R">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="mijn-library" package="RF_COIL" value="RF-ANT"/>
<element name="H1" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3">
<attribute name="POPULARITY" value="1"/>
</element>
<element name="SW1" library="SamacSys_Parts" package="PTS636SM50SMTRLFS" value="TACTWITCH">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="SCL">
<contactref element="U1" pad="1"/>
<contactref element="U3" pad="6"/>
<contactref element="R7" pad="1"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="32"/>
<contactref element="U3" pad="5"/>
<contactref element="R8" pad="1"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="+5V">
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="18"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="U3" pad="4"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="19"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="4"/>
<contactref element="U4" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U4" pad="13"/>
<contactref element="U4" pad="10"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="A12"/>
<contactref element="J1" pad="B12"/>
<contactref element="C14" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="J2" pad="8"/>
<contactref element="C16" pad="1"/>
<contactref element="J2" pad="MP1"/>
<contactref element="J2" pad="MP2"/>
<contactref element="J3" pad="8"/>
<contactref element="J3" pad="MP1"/>
<contactref element="J3" pad="MP2"/>
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="10"/>
<contactref element="J4" pad="11"/>
<contactref element="J4" pad="12"/>
<contactref element="J4" pad="13"/>
<contactref element="J1" pad="MH1"/>
<contactref element="J1" pad="MH2"/>
<contactref element="J1" pad="MH3"/>
<contactref element="J1" pad="MH4"/>
<contactref element="J2" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="LS1" pad="2"/>
<contactref element="TP13" pad="TP"/>
<contactref element="H1" pad="B3,3"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="U4" pad="14"/>
<contactref element="C11" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="U2" pad="2"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="20"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="21"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="RST">
<contactref element="C8" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="U1" pad="26"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U4" pad="6"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="2"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U4" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U4" pad="12"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U4" pad="9"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="MOSI">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="3"/>
<contactref element="U4" pad="11"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="2"/>
<contactref element="J1" pad="A5"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="B5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="B9"/>
<contactref element="J1" pad="A9"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="D1" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="EN">
<contactref element="J2" pad="3"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="J2" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="J2" pad="6"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="D0">
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="30"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="D1">
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="31"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$17">
<contactref element="J2" pad="7"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="UPDI">
<contactref element="R12" pad="1"/>
<contactref element="U1" pad="27"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$18">
<contactref element="C17" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="N$19">
<contactref element="C17" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="17"/>
</signal>
<signal name="GPIO8">
<contactref element="U1" pad="6"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GPIO9">
<contactref element="U1" pad="7"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="GPIO10">
<contactref element="U1" pad="8"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="GPIO11">
<contactref element="U1" pad="9"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="GPIO13">
<contactref element="J3" pad="7"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="GPIO12">
<contactref element="U1" pad="10"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="CD$1">
<contactref element="U4" pad="3"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="8"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="7"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="TAB">
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="7"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="GPIO24">
<contactref element="U1" pad="24"/>
<contactref element="LS1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="D3" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="GPIO25">
<contactref element="U1" pad="25"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="RTS">
<contactref element="C15" pad="1"/>
<contactref element="TP1" pad="TP"/>
<contactref element="C8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
